Material:
	Clear Acrylic Sheet
	Note: Other materials, such as Lexan may be used as alternatives

Thicknesses:
	2mm
	4mm
	6mm

Processing:
	Laser Cutting
	Note: CNC machining of the STEP file is also possible, but more expensive

Usage Conditions:
	Minimum Service Temperature: -40C
	Maximum Service Temperature: +80C
	Softening Point: 	     >110C
	Tensile Strength: 	     75MPa
	Flexural Strength:	     115MPa
	Note: Material properties may change overtime due to UV exposure

Product Details:
	Kap Case should be used together with these products:
		Khadas Edge
		Khadas Captain
		BAT-D01 Battery Module
		TS050 Touchscreen
		Edge Heatsink (optional)
		3705 Cooling Fan (optional)
		NVMe SSD (optional)
	Compatible power adapters:
		24W DC005 Adapter
		24W USB-C Adapter
	Included fasteners:
		Top Cover:
			x8 M2x5x5+10 Metal Buttons
			x8 M2 Locknuts
		LCD Screen:
			x2 M3 Star Toothed Washers
			x2 M3x12 Cross-Head Screws
			x2 M3x6x1 Nylon Washers
			x2 M3 Locknuts
		Body:
			x4 M3x8 Cross-Head Screws
			x4 M3x10x+6 Screw Extenders
			x4 M3x6 Metal Feet
