Features:

	M.2 Slot (M-Key) for 2280 NVMe SSDs
	M.2 Slot (B-Key) for 4G LTE Modules
	Nano-SIM Card Slot
	100-Mbit Ethernet Port (w/ 802.3at Power-over-Ethernet)
	10-Pin GPIO Header
	Rigid-Flex FPC Cable for connection to VIM3 / Edge-V
	Power Output: 24W (12V, 2A) via USB-C port or VIN connector
	POE Active LED
	4G Active LED

Compatibility:

	VIM3 (Full-Featured, PCIe x1 Lane)
	Edge-V (SSD-only, PCIe x4 Lane)

Documentation:

	Schematic
	Silkscreen
	Rationale
 

In The Box:

	M2X
	VIN2VIN Cable
	M2 Screws x4
	M2 Standoffs x8

* VIM3 can simultaneously use both Ethernet ports (1Gbit & 100Mbit), when connected to the M2X Extension Board.

* Edge-V can only use the SSD feature, when connected to the M2X Extension Board. The Ethernet port can receive electrical power, but no network data input. Please check Edge-V's schematic for full details.